{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["EV QRX系列小型学校剧场音响"],"not_rendered":{"external_links":2,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"EV QRX系列小型学校剧场音响","index":0,"n_rows":37,"n_cols":11,"rows_kept":37,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["EV QRX系列小型学校剧场音响"]
["序号","设备材料名称","品牌","型号","主要技术参数","数量","单位","单价","小计","注册地","备注"]
["A 扩声系统"]
["A2"," 扬声器系统"]
[1.1,"主扬声器           ","EV","QRX212/75","双12寸高输出全频音箱\n频率响应（-3dB）：75Hz ~ 15kHz\n灵敏度： 102dB LF101 HF112\n最大声压级： 135dB\n功率（被动全频）： 600W/4Ω\n功率（外置两分频）：LF 600W/4Ω; HF 75W/8Ω\n辐射角度（H×V）： 75 º×50 º",6,"只",null,null,"美国"]
[1.2,"主扬声器功放","EV","CP4000S","2通道功率放大器\n8 欧每通道900W两通道\n4 欧每通道1500W两通道\n2 欧每通道2100W两通道",3,"只",null,null,"德国"]
[1.3,"固定反听扬声器","EV","ELX112","最大中频输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： 900W 600W 380W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 500W 250W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 1700W 950W 480W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1200W 750W 420W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 1800W 1200W\n转换速率： 26V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +3.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 14.8kg",4,"只",null,null,"中国"]
[1.4,"固定反听功放","EV","Q66","最大中频输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： 900W 600W 380W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 500W 250W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 1700W 950W 480W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1200W 750W 420W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 1800W 1200W\n转换速率： 26V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +3.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 14.8kg",1,"台",null,null,"中国"]
[1.5,"流动反听扬声器","EV","ELX112","最大中频输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： 900W 600W 380W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 500W 250W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 1700W 950W 480W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1200W 750W 420W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 1800W 1200W\n转换速率： 26V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +3.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 14.8kg",2,"只",null,null,"中国"]
[1.6,"流动反听功放","EV","Q66","最大中频输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： 900W 600W 380W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 500W 250W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 1700W 950W 480W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1200W 750W 420W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 1800W 1200W\n转换速率： 26V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +3.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 14.8kg",1,"台",null,null,"中国"]
[1.7,"低音扬声器","EV","QRX218S","双18寸超低音音箱\n频率响应（-10dB）： 31Hz ~ 250Hz\n灵敏度： 102dB\n最大声压级： 139dB\n功率（被动全频）： 1200W/4Ω\n辐射角度： 全向性",2,"只",null,null,"美国"]
[1.8,"低音功放","EV","CP4000S","2通道功率放大器\n8 欧每通道900W两通道\n4 欧每通道1500W两通道\n2 欧每通道2100W两通道",1,"台",null,null,"德国"]
[6,"扬声器吊挂支架",null,null,"定制",{"$nulls":4},"定制"]
["A3","音频处理设备"]
[1,"音频处理设备","EV","DC-ONE","2进6出数字信号处理器\n带有分频、均衡、延时、压缩及限幅的功能\n带AES/EBU 数字音频输入接口\nDSP:48 kHz采样 32-Bit 浮点处理\n频率响应：10 Hz-22 kHz (+/- 0.5 dB)\n动态范围：111 dB \n输入通道:9段PEQ+31段GEQ+Delay\n输出通道:Routing+5段",2,"台",null,null,"美国"]
["A5","话筒"]
[1,"U段无线手持话筒","Sennheiser","EW 335 G3","U段无线手持式话筒系统，包括手持式话筒发射机和机架式分集接收机\n接收机技术参数：\n• 频率范围：516~865 MHz \n• 42 MHz的切换频宽，1680个可调谐的UHF频率带给你无干扰的接收\n• 增强的频率组系统，每组最多24个兼容频率\n• 有以太网接口。连网到电脑上的无线系统管理软件，可以为多通道系统带来全面的监控和专业的数据管理\n• 高品质的纯分集接收技术\n手持发射机技术参数：\n• 话筒具有显示组、通道和电池电量的背光式LCD显示屏，具备频率和功率锁定功能\n• 无线输出功率：10/30mW\n• 电池时间：>8小时\n话筒技术参数：\n• 话筒：超心型动圈型话筒；\n• 频率响应：80~18kHz\n•灵敏度：1.6 mV/Pa\n•声压级：145 dB(SPL) max.",2,"套",null,null,"德国"]
["A6","线材及接插件"]
[1,"高杆话筒架","K&M",27195,"人声话筒支架，折叠式支架腿，立杆二节，具有可延展的二节臂。支架高度：900mm~1600mm；臂长：425mm~725mm",2,"支",null,null,"德国"]
[2,"标准机柜",null,"19英寸","42U高度19英寸标准机柜、深度800mm（含滑轨、扎线支架、空面板、散热风扇、固定电源模块）",1,"套",null,null,"中国"]
[3,"防震音源机柜",null,"19英寸","18U高度19英寸标准机柜（含滑轨、空板），音源设备及周边用",1,"套",null,0,"中国"]
[4,"8路电源时序器","BE","PC800","8路时序电源，单路最大输出电流：16A",2,"台",null,0,"中国"]
[5,"多媒体地插盒",null,"定制","铝合金材质面板，4路MIC插座，1路电源，2路RCA",2,"只",null,null,"中国"]
[6,"4芯星绞话筒线",null,null,"4x0.30mm2编织屏蔽优质OFC话筒线",200,"米",null,null,"中国"]
[7,"4芯星绞音频安装线",null,null,"4x0.2mm2铝箔屏蔽优质OFC线缆",400,"米",null,null,"中国"]
[8,"2芯带护套音箱线",null,null,"2*2.5mm2绞形优质OFC带护套工程音箱线",700,"米",null,null,"中国"]
[9,"3芯卡侬公插头","Neutrik","XLR","专业XLR音频插头，用于平衡信号传输",60,"个",null,null,"瑞士"]
[10,"3芯卡侬母插头","Neutrik","XLR","专业XLR音频插头，用于平衡信号传输",60,"个",null,null,"瑞士"]
[11,"3芯卡侬母插座","Neutrik","XLR","专业XLR音频插座，用于平衡信号传输",12,"个",null,null,"瑞士"]
[12,"大三芯插头","Neutrik","TRS","专业6.35mm TRS音频插头，用于平衡信号传输",10,"个",null,null,"瑞士"]
[13,"大二芯插头","Neutrik","TS","专业6.35mm TS音频插头，用于非平衡信号传输",10,"个",null,null,"瑞士"]
[14,"莲花插头","Neutrik","RCA","专业RCA音视频插头，用于非平衡音频信号或视频信号传输",10,"个",null,null,"瑞士"]
[15,"莲花插座","Neutrik","RCA","专业RCA音视频插座，用于非平衡音频信号或视频信号传输",6,"个",null,null,"瑞士"]
[16,"音箱插头","Neutrik","Speakon","专业4芯Speakon音箱插头",20,"个",null,null,"瑞士"]
[17,"管线及安装附件","附件","定制","交钥匙工程，安装辅材满足工程需要。包括桥架，KBG钢管、PVC-U管及其它安装辅材",1,"批",null,0,"中国"]
["B 工程合计"]
[1,"设备总价：",null,null,"www.pro001.com",{"$nulls":3},"50万"]