{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["方案一"],"not_rendered":{"images":8},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"方案一","index":0,"n_rows":16,"n_cols":11,"rows_kept":16,"merged":[[0,0,0,10],[2,0,2,9]],"flags":["formulas_cached_only"]}
["北京150平米会议室扩声"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图","备注"]
["一、音响系统"]
[1,"15寸两分音全频专业音箱 ","YYAUDIO","YA15","频率响应   40Hz-18kHz\n单元组成   1×15\"(385mm)/3\" voice coil LF\n1×1\"(25mm)/1.7\" voice coil HF\n额定功率   400W RMS,1600W peak\n灵敏度   98dB 1watt/1 metre\n声压级   124dB continuous,130dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 50°\n分频点   2.2kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   560mm×525mm×800mm\n净重   29.4 kg/pc","只",2,null,0]
[2,"12寸两分音全频专业音箱 ","YYAUDIO","YA12","频率响应   50Hz-18kHz\n单元组成   1×12\"(300mm)/3\" voice coil LF\n1×1\"(25mm)/1.7\" voice coil HF\n额定功率   300W RMS,1200W peak\n灵敏度   97dB 1watt/1 metre\n声压级   122dB continuous,128 dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 50°\n分频点   2kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   480mm×465mm×725mm\n净重   20 kg/pc","只",2,null,0]
[3,"单18寸带通超低音箱 ","YYAUDIO","YA118B","频率响应   35Hz-150Hz\n单元组成   1×18＂(460mm)/4＂voice coil LF\n额定功率   600W RMS,2400W peak\n灵敏度   100dB 1watt/1 metre\n声压级   128dB continuous,134 dB peak\n额定阻抗   8 ohms nominal\n输入方式   2×Speakon NL4\n包装尺寸   835mm×645mm×750mm\n净重   49.6 kg/pc","只",2,null,0]
[4,"音箱功放","YYAUDIO","UA1100","立体声功率 8Ω:   2×550W\n立体声功率 4Ω:   2×840W\n桥接功率 8Ω:   1680W\n信噪比   ≥98dB\n转换率:   15V/μS\n阻尼系数:   >230 Nominal operating condition 1KHz/8Ω\n频响:   ±1dB Nominal operating condition 20Hz-20KHz\n\n总谐波失声:   ≤0.03% Nominal operating condition 1kHz/8Ω\n\n互调失声:   ≤0.1Nominal operating condition 60Hz/7kHz 4:1\n\n输入灵敏度   0.77V\n\n输入阻抗   20kΩ/Balancde,10kΩ/un-Balanced\n\n分离度   62dB Rated Out 1kHz/8Ω\n\nLED指示   Protect,Clip,Signal,Bridge,Stereo,Parallel,Power\n\n保护功能   Soft Start,Short Circuit,Limiter,DC Fault,AC Line Fuse,Thermal Cut\n\n散热系统   Two steps speed fan\n\n电源   AC:220-230V 50Hz/60Hz","台",2,null,0]
[5,"音箱功放","YYAUDIO","UA1500","立体声功率 8Ω:   2×750W\n立体声功率 4Ω:   2×1150W\n桥接功率 8Ω:   2300W\n信噪比   ≥98dB\n转换率:   15V/μS\n阻尼系数:   >230 Nominal operating condition 1KHz/8Ω\n频响:   ±1dB Nominal operating condition 20Hz-20KHz\n总谐波失声:   ≤0.03% Nominal operating condition 1kHz/8Ω\n互调失声:   ≤0.1Nominal operating condition 60Hz/7kHz 4:1\n\n输入灵敏度   0.77V\n\n输入阻抗   20kΩ/Balancde,10kΩ/un-Balanced\n\n分离度   62dB Rated Out 1kHz/8Ω\n\nLED指示   Protect,Clip,Signal,Bridge,Stereo,Parallel,Power\n\n保护功能   Soft Start,Short Circuit,Limiter,DC Fault,AC Line Fuse,Thermal Cut\n\n散热系统   Two steps speed fan\n\n电源   AC:220-230V 50Hz/60Hz","台",1,null,0]
[6,"调音台","YAMAHA","MG12XU","最多6个话筒 / 12 个线路输入 (4 个单声道 + 4 个立体声) / 2 编组母线 + 1 立体声母线 / 2 AUX (包括 FX）。内置高级效果器：SPX，含24组预置效。可以通过Apple iPad Camera Connection Kit / Lightning to USB Camera Adapter (连接适配器)与iPad (2或更高版本) 连接工作","台",1,null,0]
[7,"音频处理器","YYAUDIO","ES-828","音乐\n1.  音乐参量均衡:7段\n2.  音乐到主输出高通滤波器：12dB/24dB(0Hz - 303Hz)\n麦克风\n1.  有四种麦克风FBE模式：OFF  1  2  3\n2.  有麦克风压限功能\n3.  15段麦克风参量均衡\n效果\n回声：\n1.  回声低通滤波器：5.99Hz - 20.6KHz\n2.  回声高通滤波器： 0Hz - 1000Hz\n3.  回声参量均衡：3段\n4.  回声电平：0～100% \n5.  回声直达声电平： 0～100%\n6.  回声预延时：0～500ms \n7.  回声右通道预延时：0～±50% , （相对左声道）\n8.  回声总预延时： 0～500ms\n9.  回声右通道延时：0～50% , （相对左声道回声延时时间）\n10. 回声重复： 0～90%\n混响\n1.  混响低通滤波器可调范围：5.99Hz - 20.6KHz\n2.  混响高通滤波器可调范围：0Hz - 1000Hz\n3.  混响电平可调范围：0～100%\n4.  混响直达声可调范围：0～100% \n5.  回声预延时可调范围：0～200ms\n6.  混响时间可调范围：0～3000ms\n主输出（工作模式：唱歌/热舞 （自动/手动），包含除压限、延时、静音外的所有参数）\n1.  音乐电平： 0～200%\n2.  直达声电平： 0～200%\n3.  回声电平：0～200%\n4.  混响电平：0～200%\n5.  5段音乐参量均衡\n6.  压缩限幅器\n7.  左通道延时：0～50ms\n8.  右通道延时：0～50ms\n9.  左通道静音功能\n10. 右通道静音功能\n中置输出（工作模式：唱歌/热舞（自动/手动），包含除压限、延时、静音外的所有参数）\n1.  音乐电平：0～200%\n2.  直达声电平：0～200%\n3.  回声电平：0～200%\n4.  混响电平：0～200%\n5.  高通滤波器：0Hz - 303Hz\n6.  3段参量均衡\n7.  压缩限幅器\n8.  延时：0～50ms \n9.  静音功能\n超低音输出（工作模式：唱歌/热舞 与 （自动/手动），包含除压限、延时、静音外的所有参数）\n1.  音乐电平：0～400%\n2.  MIC直达声电平：0～200%\n3.  高通滤波器：12dB,Q 0.4 ～ 1.5,/Bessel 24dB/Butterworth 24dB/Link Riley 24dB/USER 12dB/USER 24dB (0Hz - 303Hz)\n4.  低通滤波器：12dB,Q 0.4 ～ 1.5,/Bessel 24dB/Butterworth 24dB/Link Riley 24dB/USER 12dB/USER 24dB (0Hz - 303Hz)\n5.  3段参量均衡 \n6.  压缩限幅器\n7.  延时：0～50ms\n8.  静音功能\n后置输出（工作模式：唱歌/热舞 与 （自动/手动），包含除压限、延时、静音外的所有参数）\n1.  音乐电平：0～200% \n2.  直达声电平：0～200% \n3.  回声电平：0～200%\n4.  混响电平：0～200%\n5.  高通滤波器：0Hz - 303Hz\n6.  3段参量均衡 \n7.  压缩限幅器\n8.  左通道延时：0～50%\n9.  右通道延时：0～50%\n10. 左通道静音：静音/非静音\n11. 右通道静音：静音/非静音","台",1,null,0]
[8,"一拖二话筒","YYAUDIO","T8","接收机 RECEIVER\n接收频率Frequency Ranges：UHF600-900MHz\n频率稳定度Frequency Stability：±0.002%（用优于15ppm石英晶体锁定）\n灵敏度Sensitivity（peak deviation）：10μV\n鄰道幹擾比F/N Ratio：>8odB\n鏡像干擾比P/N Ratio：>80dB\n信噪比S/N Ratio：>90dB\n扩展比Dilation Ratio：1：2\n音频输出AF Output Voltage（at peak deviation 1kHz AF out）：可调0 ~ 300mV\n接收频道Channels：2路 \n输出接口 Output jack：6.3不平衡混合口 \n电源电压Power Supply：DC 13V-500mA(50Hz\n功耗Power Supply：6W\n天线Antenna：外置天线\n动能范围Dynamic frequency range：>100dB\n综合失真T.H.D：<0.5%\n工作温度Temperature Range：-10℃ ~ 50℃\n\n发射机 TRANSMITTER\n发射频率Frequency Ranges： UHF600-900MHz\n频率稳定度Frequency Stability：0.002%（用优于15ppm石英晶体锁定）\n发射功率 RF Power：30mW\n电流损耗 Cuttent Consumption：< 主波40dB\n制式Modulation Mode：调频FM\n调偏度Deviation Range：±20KHz\n压缩比Compress Ratio：2.1\n拾音器Microphone Head：超心型动圈式\n电池Battery Type：两节5号1.5V碱性电池\n天线 Anternna：外置式 Exterior Antenna\n频率响应 Frequency Response：50Hz ~ 15KHz\n有效距离Receiver distance：50米（理想环境下）","套",1,null,0]
[9,"壁挂音箱支架",{"$nulls":3},"套",4,null,0]
[10,"辅材",null,null,"音箱头、莲花线、莲花转3.5等","批",1,null,0]
[11,"音箱线","高强信",null,"2.0平方","米",200,null,0]
[12,{"$nulls":7},0]
[null,"以上价格不含税不含运费"]