{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["方案一"],"not_rendered":{"images":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"方案一","index":0,"n_rows":8,"n_cols":11,"rows_kept":8,"merged":[[0,0,0,10],[2,0,2,10],[7,1,7,7]],"flags":["formulas_cached_only"]}
[" 设备清单"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","图样","备注"]
[]
[1,"双十八寸低音音箱","JBL","MRX628S","双18“大功率低音炮\nMRX628S是一款紧凑型高功率超低音扬声器系统，在前置式通风外壳中包含双2044H 457 mm（18 in）低音扬声器。外壳设计为最小的正面区域。它还采用直立式配置，以便在顶部方便地堆叠全范围外壳，而无需额外的杆。\n特征\n双18英寸，2044H驱动器，用于扩展低频输出\n大通风口可减少失真\n垂直方向，便于地面堆叠\n坚固的DuraFlex™外壳饰面\n应用\n现场表演场地\n移动和固定DJ系统\n规格\n频率范围（-10 dB）35 Hz - 250 Hz\n频率响应（±3 dB）40 Hz - 250 Hz\n输入连接模式可在内部配置，+ 1 / -1或+ 2 / -2\n推荐的Crossover 80 - 120 Hz，24 - 48 dB / octave\n额定功率（连续/程序/峰值）1000 W / 2000 W / 4000 W，\n2小时  800 W / 1600 W / 3200 W，100小时\n最大SPL 133 dB SPL连续（139 dB SPL峰值）\n系统灵敏度（1w @ 1m）97 dB SPL; 103 dB SPL\nLF驱动器2 x JBL 2044H 457 mm（18 in）低音扬声器\n标称阻抗4欧姆\n外壳矩形，18毫米，桦木胶合板\n完成黑色DuraFlex™表面处理\n格栅粉末涂层，黑色，16规格穿孔钢，带声学透明黑色屏幕背衬\n输入连接器Neutrik®Speakon®NL-4（x2）\n尺寸（高x宽x深）1095毫米x 535毫米x 700毫米（43英寸x 21.0英寸x 27.5英寸）\n净重55千克（121磅）","只",4,null,0,null," "]
[2,"2*1000W功放","CROWN","PX4000","支持立体声/并联/单声道桥接模式；用户可选择的输入灵敏度：0.775V和1.4V；RCA和XLR输入接口；Speakon和喇叭接线柱输出接口；2个增益控制旋钮，一个电源开关，一个电源LED灯，2组6个LED灯分别表示对应单声道处于工作、削波和故障状态；防止短路、空载、开/关机噪音、射频干扰保护电路\n立体声4Ω：1350W/ch，立体声8Ω/ch：1000W；\n桥接8Ω：2700W；\n声道：2ch；\n灵敏度：0.775V或者1.4V；\n信噪比：>100dB；\n谐波失真：<=0.5%；\n互调失真：<=0.35%；\n频率响应：20Hz-20KHz；\n串音：1KHz：-75dB； 20KHz：-59dB\n；阻尼系数：>200（10Hz-400Hz，8Ω负载）；\n外形尺寸：89*482*366mm；\n净重：19.5Kg","台","2",null,0]
[1,"双十八寸低音音箱","JBL","SRX728S","SRX728S是一款高功率超低音扬声器系统，包含两个2268H钕磁铁，获得专利的差分驱动器®，18英寸低音扬声器，位于前置式通风外壳中。\n特征\n双18英寸，2268H差分Drive®低音扬声器，用于扩展低频输出。\n大通风口区域可减少变形。\n规格\n额定功率1600 W / 3200 W / 6400 W.\n频率范围27 Hz - 220 Hz（-10 dB）\n外形尺寸\n（高x宽x深）610毫米×1067毫米×838毫米\n（24英寸x 42英寸x 33英寸）\n频率响应33 Hz - 220 kHz（±3 dB）\n净重76千克（166.5磅）","只",4,null,0]
[2,"功率放大器","CROWN","XTi6002A","2*1200W 8欧，2*2100W 4欧，1*6000W 4欧，内置数字处理","台",2,null,0]
[3,{"$nulls":7},131820]