{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["方案"],"not_rendered":{"images":4,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"方案","index":0,"n_rows":8,"n_cols":11,"rows_kept":8,"merged":[[0,0,0,10],[2,0,2,9]],"flags":["formulas_cached_only"]}
["音响方案清单"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图","备注"]
["一、音响系统"]
[1,"音箱","TURBOSOUND","TCX122","扬声器单元组成\n低频：12” × 1；高频：1” × 1\n频率响应\n100 Hz – 18 kHz / ± 3dB；\n68 Hz – 20 kHz / -10dB\n覆盖角度\n90°H × 60°V (可旋转)\n功率 (连续/峰值)\n300W / 1200W\n最大声压级（连续/峰值）\n122dB / 128dB\n分频点\n被动分频 2kHz\n标称阻抗\n8 Ω\n接插件\nNL4 × 2，接线排端口\n尺寸（高×宽×深）\n552 × 406 × 368 mm\n净重（kg/lbs）\n18.3 / 40.2\n\n\n特性\n· 适合流动演出或固定安装应用\n· 可旋转会聚式椭圆形号角(CEW™)\n· Speakon NL4母座及接线排端口\n· 兼容万向(Omnimount™)吊挂件\n· EASE GLL数据库支持","只",4,null,0]
[2,"功放","YYAUDIO","UA2000","1000W×2/8Ω 1750W×2/4Ω\n频响：20Hz-20kHz(+0/-1dB)\n总谐波失真：≤0.15％\n信噪比：≥100dB\n阻尼系数：≥500\n转换速率：≥10V/μs\n输入灵敏度：0.775V/1.0V/32dB\n输入阻抗：20kΩ/10kΩ\n电压增益（8Ω时）：36.0dB\n功放拓扑类别：ClassD\n冷却：Air flow from front to  rear\n","台",2,null,0]
[3,"调音台","Soundcarft","FX16II","• 数码音响的音质\n• 最多可接26组输入信号\n• 16组话筒线路输入\n• 专利设计的UltraMic前置放大器\n• 内置广播级的Lexicon莱思康效果器，双效果，可编程，可修改参数\n• 16组直接输出，可选择推子前或后，用作多轨录音或效果送出\n• 3段英国风味的均衡器，中频可选项\n• 18dB的高通滤波器\n• 4组母线\n• 4组立体声输入\n• 100mm专业推子\n• 48幻像供电\n• 通道输入、编组和主输出都设有插入点\n• 独立音量控制的单声道输出\n• 接线通盘可以改变位置，配合不同的安装方式\n• 可以安装在19\"机柜","台",1,null,0]
[4,"均衡器","DBX",1231,"双通道31段1/3倍频程的\"均衡。各频段的中心频率均符合1SO国际认可的规格，+/-12dB输入增益调整范围，以及可切换的40H/18dB倍频程低通滤波器。其他各种特性还包括45mm推子；可选择的+/-6dB或+/-l5dB提升/衰减范围，以便进行更精确的增益调整；XLR、排状接线端子和1/4\"RS平衡接口适应各种安装需要；用于低噪声工作的平衡式输人和输出；以及消除交流噪声的机箱/信号接地悬浮功能。12系列直观化的设计令操作更加容易。","台",1,null,0]
[{"$nulls":8},53400]