{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["meyersound小型学校剧场音响"],"not_rendered":{"external_links":9,"defined_names":52},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"meyersound小型学校剧场音响","index":0,"n_rows":169,"n_cols":8,"rows_kept":169,"merged":[[0,0,0,6],[1,1,1,2],[2,1,2,2],[3,1,3,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,0,146,0],[136,1,146,1],[147,0,149,0],[147,1,149,1],[150,0,156,0],[150,1,156,1],[157,0,161,0],[157,1,161,1],[162,0,165,0],[162,1,165,1],[166,1,166,2],[167,1,167,2],[168,0,168,4]],"flags":["formulas_cached_only"]}
["meyersound小型学校剧场音响"]
["序号","名称",null,"单位","数量","成本价合价","承诺品牌","备注"]
["A","音乐厅音响设备清单"]
[1,"中央声道扬声器1",null,"组",1,null,"MeyerSound（UOQ-1P)"]
[2,"中央声道扬声器2 ",null,"组",1,null,"MeyerSound(UPQ-2P）"]
[3,"左右声道扬声器",null,"组",2,null,"MeyerSound(UPQ-1P）"]
[4,"舞台后观众区补声",null,"组",1,null,"MeyerSound(UPJ-1P)","每组3只，共3只"]
[5,"台唇补声全频扬声器",null,"组",1,null,"MeyerSound(UPM-1P)","每组6只，共6只"]
[6,"环绕声扬声器 ",null,"只",12,null,"MeyerSound(UPM-1P)"]
[7,"舞台流动返送扬声器",null,"只",4,null,"MeyerSound(UM-100P)"]
[8,"功率放大器",null,"套",1,null,"MeyerSound(RMS)","功放网络远程遥控检测系统及软件"]
[8.1,"左中右声道扬声器功率放大器",null,"台",0]
[8.2,"舞台后观众区补声功率放大器、台唇补声功放",null,"台",0]
[8.3,"环绕声扬声器功率放大器",null,"台",0]
[8.4,"舞台流动返送扬声器功率放大器",null,"台",0]
[9,"数字调音台",null,"套",1,null,"DIGICO（SD9-2P)"]
[10,"监听耳机",null,"副",1,null,"AKG(K240)"]
[11,"声控室监听音箱",null,"只",3,null," YAMAHA (HS50M)"]
[12,"音频工作站",null,"套",1,null,"Protools (苹果主机加Protools)"]
[13,"双通道图示均衡器 ",null,"台",4,null,"KT(DN370)"]
[14,"数字效果处理器 ",null,"台",1,null,"T.C Electronics、LEXICON(MONE)"]
[15,"数字效果混响器",null,"台",1,null,"T.C Electronics(M350)"]
[16,"数字压缩/限幅器",null,"台",2,null,"KT(Square ONE Dynamics)"]
[17,"信号分配器",null,"项",1,null,"KT(Square ONE splitter)","每项6台，共6台"]
[18,"CD机",null,"台",1,null,"DENON(DN-C615)"]
[19,"MD机",null,"台",1,null,"TASCAM(MD02B)"]
[20,"硬盘录放机",null,"套",1,null," 360Systems(DR600E)"]
[21,"双通道接收机",null,"台",8,null,"SHURE(UHF-R)"]
[22,"腰包发射器 ",null,"台",16,null,"SHURE(UR1)"]
[23,"无线手持发射话筒",null,"台",8,null,"SHURE(UR2/Beta58)"]
[24,"领夹话筒 ",null,"支",8,null,"SHURE(WCB6T）"]
[25,"头戴话筒 ",null,"支",8,null,"SHURE（WBH53T)"]
[26,"天线分配器",null,"台",2,null,"SHURE(UA845)"]
[27,"远程天线",null,"副",4,null,"SHURE(UA874WB)"]
[28,"小型心形麦克风",null,"支",1,null,"SHURE(SM57)"]
[29,"小型心形麦克风",null,"支",1,null,"SHURE(SM81)"]
[30,"小型可切换麦克风",null,"支",1,null,"audio-technica(AT)"]
[31,"小型麦克风的可调节高度带有旋转和直线伸缩管的支架",null,"支",11,null,"定制"]
[32,"用于小型麦克风的ORTF立体声吊杆",null,"支",1,null,"定制"]
[33,"电缆吊架，用于小型麦克风",null,"支",11,null,"定制"]
[34,"电容式心型麦克风",null,"支",6,null,"SHURE(SM27) "]
[35,"电容式超心型麦克风",null,"支",4,null,"SHURE(SM 87A) "]
[36,"用于电容麦克风的电缆挂钩",null,"个",10,null,"SHURE(44A 16928) "]
[37,"电容式手持麦克风",null,"支",2,null,"SHURE(SM86)"]
[38,"大振膜电容式麦克风",null,"支",1,null,"AKG(C3000)"]
[39,"大振膜电容式麦克风, 可切换",null,"支",1,null,"SHURE (KSM44A)"]
[40,"手持麦克风，用于发言\n\n\n\n\n\n\n\n\n",null,"支",4,null,"SHURE(BET58) "]
[41,"手持麦克风, 用于乐器",null,"支",4,null,"SHURE (BETA57A)"]
[42,"用于鼓的麦克风设置（低音鼓的麦克风）",null,"套",1,null,"SHURE (PGDMK6)"]
[43,"麦克风支架，带长杆话筒臂",null,"个",15,null,"K&M(27195)"]
[44,"麦克风电缆，高质量及灵活性，10m长",null,"个",30,null,"森格(定制）"]
[45,"麦克风电缆，高质量及灵活性，20m长",null,"件",20,null,"森格(定制）"]
[46,"麦克风电缆，用于悬挂麦克风，20m长",null,"件",12,null,"森格(定制）"]
[47,"立体声麦克风电缆，用来悬挂环绕麦克风，20m长",null,"件",2,null,"森格(定制）"]
[48,"3节话筒架 ",null,"支",6,null,"K&M（25900）"]
[49,"工程安装中其它辅助材料",{"$nulls":5},"以下列项由投标人自行考虑数量并报价，该部分报价为一次性固定报价，中标后不得调整"]
[49.1,"6芯音箱线 ",null,"项",1,null,"森格（6*25mm2）"]
[49.2,"2芯音箱线 ",null,"项",1,null,"森格(2×2.5mm2)"]
[49.3,"2芯音箱线 ",null,"项",1,null,"森格(2×4mm2）"]
[49.4,"8通道信号缆",null,"项",1,null,"森格（定制）"]
[49.5,"12通道信号缆",null,"项",1,null,"森格（定制）"]
[49.6,"网线",null,"项",1,null," AMP（超五类线）"]
[49.7,"50欧射频电缆",null,"项",1,null,"森格(50Ω）"]
[49.8,"复合视频电缆",null,"项",1,null,"森格(75Ω-5）"]
[49.9,"DVI电缆",null,"项",1,null,"秋叶原（定制） "]
[{"v":49.1,"d":"49.10"},"VGA电缆",null,"项",1,null," 成丰（5BNC)"]
[49.11,"控制线",null,"项",1,null," 成丰"]
[49.12,"功放远程监控专用电缆",null,"项",1,null," AMP (6类）"]
[49.13,"模拟音频电缆",null,"项",1,null,"森格 （2×0.3mm2）"]
[49.14,"工程话筒电缆",null,"项",1,null,"森格 （4×0.3mm2）"]
[49.15,"成品话筒线",null,"项",1,null,"森格 （4×0.3mm2）"]
[49.16,"8信道音频电缆",null,"项",1,null,"森格（8信道音频电缆） "]
[49.17,"光纤",null,"项",1,null," AMP（多模）"]
[49.18,"电源线1",null,"项",1,null,"  远东（3×4m㎡/3×2.5m㎡）"]
[49.19,"电源线2",null,"项",1,null," 远东（3×6m㎡）"]
[{"v":49.2,"d":"49.20"},"电缆1",null,"项",1,null," 远东（4×25+1×16m㎡）"]
[49.21,"电缆2",null,"项",1,null," 远东（4×50+1×25m㎡）"]
[49.22,"视频插接件（BNC/DVI/VGA/莲花等)",null,"项",1,null,"NEUTEIK(镀银 接触电阻﹤5毫欧 3芯)"]
[49.23,"内通专用电缆",null,"项",1,null,"成丰（与选用内通系统形式配套）"]
[49.24,"8通道多芯插头（公/母）",null,"项",1,null,"NEUTEIK(镀镍 接触电阻﹤0.05欧)"]
[49.25,"12通道多芯插头（公/母）",null,"项",1,null,"NEUTEIK(镀镍 接触电阻﹤0.05欧)"]
[49.26,"扬声器插头",null,"项",1,null,"NEUTEIK(镀镍 接触电阻﹤0.2欧 4芯)"]
[49.27,"扬声器插座",null,"项",1,null,"Neutrik "]
[49.28,"卡侬插（公） ",null,"项",1,null,"Neutrik "]
[49.29,"卡侬插（母） ",null,"项",1,null,"Neutrik "]
[{"v":49.3,"d":"49.30"},"立体声直插 ",null,"项",1,null,"Neutrik "]
[49.31,"RCA插头 ",null,"项",1,null,"Neutrik "]
[49.32,"电源插头 ",null,"项",1,null,"公牛 "]
[49.33,"电源插排 ",null,"项",1,null,"公牛 "]
[49.34,"2*48通道跳线盘 ",null,"项",1,null,"Canare "]
[49.35,"软跳线（30cm长） ",null,"项",1,null,"Canare "]
[49.36,"8通道I/O盒 ",null,"项",1,null,"广利德 （定制）"]
[49.37,"12通道I/O盒 ",null,"项",1,null,"广利德 （定制）"]
[49.38,"8通道成品扇尾线",null,"项",1,null,"森格（镀镍 接触电阻﹤0.1欧 2m）"]
[49.39,"12通道成品扇尾线",null,"项",1,null,"森格（镀镍 接触电阻﹤0.1欧 2m）"]
[{"v":49.3999999999999,"d":"49.40"},"流动机柜 ",null,"项",1,null,"图腾 （标准机柜）"]
[49.41,"固定机柜 ",null,"项",1,null,"图腾 （标准机柜）"]
[49.42,"1U盲板 ",null,"项",1,null,"广利德 "]
[49.43,"2U盲板 ",null,"项",1,null,"广利德 "]
[49.44,"音箱吊挂件 ",null,"项",1,null,"国产优质"]
[49.45,"金属桥架",null,"项",1,null,"振大（国标 50×50、100×100、300×100等规格）"]
[49.46,"电线钢导管",null,"项",1,null,"朋正（国标 JDG25-32规格）"]
[49.47,"音视频系统配电箱",null,"项",1,null,"国产优质(国标 按照图纸要求制作）"]
[49.48,"摄像头云台支架",null,"项",1,null,"广利德（与所选用摄像头云台配套) "]
[49.49,"内通插座",null,"项",1,null,"定制"]
[{"v":49.4999999999999,"d":"49.50"},"插座盒",null,"项",1,null,"广利德(定制）"]
[49.51,"综合插座箱",null,"项",1,null,"广利德（定制） "]
[49.52,"扩声及视频系统操作台",null,"项",1,null,"广利德（定制） "]
[49.53,"调音台工作照明灯",null,"项",1,null,"与调音台品牌相同"]
[49.54,"无线话筒保管箱",null,"项",1,null,"国产优质（定制）"]
[49.55,"有线话筒保管箱",null,"项",1,null,"国产优质"]
[49.56,"舞台监督台",null,"项",1,null,"广利德 （定制）"]
[49.57,"其它辅材",null,"项",1,null,"国产优质（定制）"]
[49.58,"时序电源",null,"项",1,null," LAX （8路）"]
["B","音乐厅内部通讯设备清单"]
[1,"内部通讯矩阵",null,"台",1,null,"Clear-Com( SB-704)"]
[2,"内部通讯主机站",null,"台",1,null,"Clear-Com(MS-702)"]
[3,"内部通讯扩展",null,"台",1,null,"Clear-Com"]
[4,"双通道通讯分机",null,"台",3,null,"Clear-Com(RM-702)"]
[5,"鹅颈话筒",null,"台",5,null,"Clear-Com(GM-18)"]
[6,"双通道腰包机",null,"台",8,null,"Clear-Com（RS-601)"]
[7,"单耳通话耳机",null,"副",12,null,"Clear-Com(CC-60)"]
[8,"无线腰包机充电器",null,"个",4,null,"Clear-Com (WTR4C+WTR-BAT)"]
[9,"双通道无线通讯基站",null,"台",1,null,"Clear-Com(WBS-680/A2)"]
[10,"双通道无线腰包机",null,"个",4,null,"Clear-Com(WTR-680/A2) "]
[11,"矩阵式继电器组切换器",null,"台",1,null," TOA(FS-900MX) "]
[12,"定压功放",null,"台",4,null," TOA(A-1120MK2) "]
[13,"6W天花喇叭",null,"只",40,null," TOA(PC-1868D) "]
[14,"6W调音器",null,"个",20,null," TOA(AT-064H) "]
[15,"定压功放",null,"台",2,null," TOA(A-1240MK2) "]
[16,"30W宽音域喇叭",null,"只",10,null," TOA(BS-1030B) "]
[17,"对讲机机站 ",null,"个",1,null," 建伍(TKR-750/850)  "]
[18,"充电器 ",null,"个",12,null,"建伍(KSC-35) "]
[19,"电源 ",null,"项",1,null,"SEMER(PS818)  ","每项4台，共4台"]
[20,"控制用笔記本电脑 ",null,"台",1,null,"Dell( Inspiron  15R)"]
["C","音乐厅内部监视设备清单"]
[1,"摄象机","挑台"]
[null,null,"3CCD彩色视频摄像机 ","台",1,null," BOSCH(LRC 0485)"]
[null,null,"摄像机电缆 ","项",1,null," BOSCH(定制）","每项1根，共1根"]
[null,null,"摄像机适配器","台",1,null," BOSCH(定制）"]
[null,null,"广角变焦镜头 ","台",1,null," BOSCH(定制）"]
[null,null,"云台","台",1,null,"定制"]
[null,null,"观众厅及舞台区"]
[null,null,"3CCD彩色视频摄像机","台",2,null," BOSCH（LTC5136)"]
[null,null,"摄像机电缆","项",1,null," BOSCH(定制）","每项2根，共2根"]
[null,null,"摄像机适配器","台",2,null," BOSCH(定制）"]
[null,null,"广角变焦镜头 ","台",2,null," BOSCH(定制）"]
[2,"监视器","24〞液晶显示器 ","台",3,null," SONY(KDL-24EX520)"]
[null,null,"32〞液晶显示器","台",9,null," SONY(KDL-32W650A) "]
[null,null,"显示器吊架","套",12,null,"国产"]
[3,"控制室内设备","摄像机控制器","台",1,null," BOSCH(LTC5136)"]
[null,null,"硬盘录像机 ","台",1,null,"大华(DH-DVR0804HG-S) "]
[null,null,"多媒体服务器","台",1,null,"SONY"]
[null,null,"视频控制软件 ","套",1,null,"SONY"]
[null,null,"视频信号跳线板 ","项",1,null,"定制"]
[null,null,"设备操作控制台 ","台",1,null,"广利德(定制）"]
[null,null,"网络交换机","套",1,null,"Dlink（1016）  "]
[4,"有线电视信号分配  （与弱电配合）","八通道有线电视解调器","台",1,null,"PBI"]
[null,null,"有线电视混合器","台",1,null,"PBI"]
[null,null,"有线电视放大器","台",1,null,"PBI"]
[null,null,"分配器","项",1,null,"歌华"]
[null,null,"分支器","项",1,null,"歌华"]
[5,"舞台提示系统","提示灯系统","套",1,null,"LEMUSE"]
[null,null,"子母钟系统（三联播出母钟）","套",1,null,"北极星（BKS2-1) "]
[null,null,"三联播出子钟","台",4,null,"北极星(YZD516) "]
[null,null,"播出时钟控制器","台",1,null,"北极星（BKS2-1-1) "]
[null,"调试费用",null,"项",1]
[null,"其他费用",null,"项",1]
["合计：",{"$nulls":4},"450万"]