{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["方案三"],"not_rendered":{"images":6},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"方案三","index":0,"n_rows":14,"n_cols":10,"rows_kept":14,"merged":[[0,0,0,9],[2,0,2,9],[13,0,13,7]],"flags":["formulas_cached_only"]}
["JBL LS80系列方案"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
["一、影院扩声系统"]
[1,"主音箱","JBL","LS80","音箱类型：三分频落地式扬声器 \n输出功率：200W \n低音单元：2×200英寸\n高音单元：50英寸 \n阻抗：6Ω \n灵敏度：90dB \n分频频率：2.5KHz，8kHz \n频率响应：35Hz-40kHz \n产品尺寸：1104*259*418mm \n产品重量：35.6kg/只  \n","只",2]
[2,"环绕音箱","JBL","L820","主要参数 扬声单元 超高频驱动单元: 3/4寸 (19mm) Mylar 球顶铝铸底盘，安装在 Bi-Radial(双辐射)号角中 \n高频换能器: 1寸(25mm) 纯钛球顶(安装在JBL EOS导波管中)铝铸底盘 \n低频换能器: 6寸(130mm) PolyPlas 锥盆，带橡胶悬边、铝铸底盘、HeatScape 马达结构、对称几何磁场设计(SFG)、超大 Kapton 音圈、磁短路环\n频响范围 55Hz-40kHz\n灵敏度 90dB\n阻抗 8Ω\n功率 最大建议功率放大器功率: 150W \n功率容量(连续值/峰值功率): 75W/300W\n音箱接口 RCA接口\n音箱材质 木质\n外观色 黑\n尺寸 311×391×127 mm\n重量 8.6Kg","只",2]
[3,"中置音箱","JBL","LS center","音箱类型 三分频中置扬声器 \n输出功率 150W \n低音单元 2×165英寸 \n高音单元 50英寸 \n阻抗 6Ω \n灵敏度 88dB \n分频频率 2.5KHz，9kHz \n频率响应 50Hz-40kHz \n产品尺寸 672×217×235mm \n产品重量 14.4kg/只 \n","只",1]
[4,"低音音箱","JBL","LS120P","音箱类型：12寸有源低音炮 \n输出功率：400W \n低音单元：300英寸 \n频率响应：25Hz-150Hz \n外观参数 产品尺寸：487*375*425mm \n产品重量：25.8kg/只 ","只",1]
[5,"AV功放","DENON","AVR-X3100","颜色 银色\n影院种类 有线\n产品类别 AV功放\n音响\n信噪比 100 dB（IHF-A 计权，DIRECT 模式）\n声道系统 7.2 声道\n播放功能\nUSB 有\n端口\n机身输入 HDMI（前置1个）、分量、复合（视频）、模拟音频、数字光纤、数字同轴\n机身输出 HDMI(监视器\\区域2、模拟音频、耳机、音频前级输出\n麦克风 不支持\n材质\n机箱材质 金属\n尺寸\n包装尺寸（长宽高） 530W*260H*480Dmm\n主机尺寸（长宽高） 434W x 167H x 379D mm\n重量\n包装重量 13.1KG\n主机重量 10.7KG\n其他功能\n闹钟\\开关机 支持\n特性\n特性功能 1.所有7 个声道完全分立、同品质和等功率. 2. 高级多声道环绕声：DTS-Neo：X、Audyssey DSX、Dolby ProLogic IIz. 3.网络、AirPlay 和Denon Remote App. 4.HDMI 完全支持下一代4K 显示器并配备了7 个输入和2个输出.","台",1]
[7,"蓝光DVD","PIONEER","BDP160","视频功能： 视频文件：DivX plus HD/mpg/mp4/ts/m2ts/m4v/avi/flv/mov/3gp/wmv/mkv\n视频特性：\n148.5MHZ/12-bit数模转换器\nDeep Colour 36比特深色域\nx.v.colour\nHDMI 1080p 24HZ输出\n3D视频播放\n\n光碟格式： Blu-ray Disc(BD-ROM/BD-RE/BD-R,8CM BD-R/BD-RE)\nDVD(DVD-Video/DVD-R/DVD+R/DVD-RW/DVD+RW)\nVideo CD\nCD(CD-DA/CD-R/CD-RW/CD-EXTRA/CD-GRAPHICS/dts-CD)\nAVCHD/AVCRED\n\n音频功能： 音乐文件及解码：MP3/WMA/MPEG4 AAC/FLAC/LPCM/Monkey's Audio\n24-bit/192kHZ数模转换器\nDTS-HD Master Audio 解码器\nDolby TrueHD解码器\n音频修正连接\n\n输入输出端口： HDMI输出 x1\n同轴音频输出 x1\nUSB连接 x1\nLAN端口 x1\n模拟音频输出\n\n其它功能： 图片文件：JPEG/MPO(3D)/PNG/GIF\n\n电源性能： AC110-240MV，50/60Hz\n\n产品尺寸： 435*58*250mm\n\n产品重量： 2.7kg","台",1]
[8,"硬盘",null,null,"可插到DVD USB口存储播放影片用","个",1,null,null,"自备"]
[9,"HDMI线",null,null,"10米","条",1,null,null,"自备"]
[10,"音响线","高强信",null,"3平方","米",200,null,null,"自备"]
[11,"投影机吊架",null,null,"0.6米以上","个",1,null,null,"自备"]
["合计",{"$nulls":7},62000]